A circuit board

Description automatically generated

*Figure 1: The circuit shown above is that for this lab.*

4) The differences result from the frequency while having the same aptitudes have different forms. Specifically, the sine wave generator is producing an analogue signal versus a digital signal the Arduino produces. This results in a Sine Wave and Square Wave, both respective to what they are being created by resulting in the sound differences.